**Upgrading Process Software V2.7.42**

Before starting upgrade the CC, is there some considerations to be made.

If the CC is with older software – ex. V1.x.x.tar - then both the process have to be carried out, as described in **Step 1** and **Step 2**.

If the CC is with software ex. V2.1.x.tar - or later - then only the process described in **Step 2** have to be carried out.

Follow below description careful.

**Step 1:** require a separate Mini SD card of max. 2GB (not a HC card)

Upgrade from V1.x.x to V2.1.35:

Download the dlcc\_2.1.35.zip folder to a Mini SD card.

Unzip the folder, so that the files”cc-2.0.0.tar” and”dlcc-2.1.35.tar” are visible and separate in the root.

Insert the Mini SD card

Start the upgrade process via Setup:

1. Press the Setup button at left side under the front with either a pencil or with the end of another small object.
2. Press - ”Software”
3. Press - ”Start Upgrade”
4. Press - ->”Upgrade Software Now!”

NOTE:

\*1: The upgrade will run two times

\*2: If upgrading from version 1.0.2282, all units must be factory reset and re-installed/configured.

**Step 2:** require a separate Mini SD card of max. 2GB (not a HC Card)

Upgrade from V2.1.x to latest version – in this case V2.7.42

Download the dlcc- 2.7.42zip file to a Mini SD card

Unzip the file so that the “dlcc-2.7.42.tar” is visible and separate in the root

Insert the Mini SD card

Start the upgrade process via Setup:

1. Press the Setup button at left side under the front with either a pencil or with the end of another small object.
2. Press - ”Software”
3. Press - ”Start Upgrade”
4. Press - ->”Upgrade Software Now!”